|  |  |
| --- | --- |
| **FORNAX™ ePlanCheck Rule** | |
| **Building Code Information** | |
| **Rule ID** | WTR 8.3.6 |
| **Rule Name** | Double check valves for drinking fountains or water coolers |
| **Chapter** | 4 Fittings and Appliances |
| **Section** | 4.2 Fittings |
| **Handbook** | Code of Practice for Water Services  Incorporating Amendment No. 1 and No. 2– CP 48 : 2005 |
| **Author** | Joemar M. Alberto |

Conceptual Graph

