|  |  |
| --- | --- |
| **FORNAX™ ePlanCheck Rule** | |
| **Building Code Information** | |
| **Rule ID** | SSW 1.2.2 (c) (iii) |
| **Rule Name** | Minimum trench width is 750 mm if the sewerage pipe less is than 3000 mm deep |
| **Chapter** | Part 1 Planning & Design Requirements For Development Works |
| **Section** | 1.2 Planning Requirements |
| **Handbook** | Code of Practice on Sewerage and Sanitary Works Addendum No. 2 - Nov 2004 |
| **Author** | Carl Mark Balajadia |

|  |
| --- |
| **Conceptual Graph** |
|  |